The number of *octaves* in a signal is defined as

where *n* is the number of points in the zero-padded time series.

The total number of scales in the CWT will be

.

The value of each *scale*, *ai*, is given by

where

.

Therefore, *scale* varies from to .